To construct a BRINTAF loop for normalizing the **QV:7MALP** (Quantum Variable: 7-Multi-Axis Logic Protocol) prior to the **Druskel Phase**, you must ensure the synchronization of the sub-vectors before the phase-drift threshold is reached.

Below is the procedural logic flow designed for high-latency quantum environments.

### The BRINTAF Loop Structure
**B**ypass -> **R**ecalibrate -> **I**nterlace -> **N**ormalize -> **T**ransmit -> **A**ccelerate -> **F**inalize

---

#### 1. Bypass (Initialization)
Isolate the QV:7MALP from the primary manifold to prevent cascading errors during the pre-Druskel instability.
*   *CMD:* `SHIFT_ISOLATE --target QV:7MALP --mask 0xFF00`

#### 2. Recalibrate (Frequency Alignment)
Align the harmonic oscillators of the 7-axis to the projected Druskel carrier wave frequency. This prevents phase-clipping.
*   *CMD:* `PHASE_SYNC --set_target [Druskel_Carrier_REF]`

#### 3. Interlace (Data Weaving)
Integrate the secondary telemetry bits into the 7MALP structure. This provides the redundancy required for the Druskel transformation.
*   *CMD:* `INTERLACE_BUFFER --stream [Telemetry_B] --dest QV:7MALP`

#### 4. Normalize (The Core Loop)
This is the heart of the operation. Execute 7 iterations to stabilize the logic gate variance within a ±0.03 margin.
*   **Loop Syntax:**
    ```pseudo
    FOR i = 1 TO 7:
       APPLY vector_median_filter(QV[i])
       ELIMINATE ghost_nodes(QV[i])
       IF variance > 0.03: RE-LOOP 1
       ELSE: CONTINUE
    ENDFOR
    ```

#### 5. Transmit (Handshake)
Push the normalized variable into the transition sub-buffer. Do not release to the main cluster yet.
*   *CMD:* `BUFFER_COMMIT --source Normalized_QV:7MALP --destination Sub_Buffer_Alpha`

#### 6. Accelerate (Pre-Druskel Loading)
Ramp up the clock speed of the buffer to match the intake velocity of the impending Druskel Phase.
*   *CMD:* `CLOCK_STRETCH --ratio 1.25:1`

#### 7. Finalize (Exit Condition)
Verify checksums and trigger the Druskel bridge interface.
*   *CMD:* `INTERFACE_OPEN --protocol DRUSKEL_PHASE_GATE`

---

### Important Safety Constraints:
*   **Entropy Threshold:** If the normalization variance exceeds 0.08 during the BRINTAF process, **abort the loop immediately.** Attempting to force the Druskel phase with an un-normalized QV:7MALP will result in a logic inversion error (L-ERR:78).
*   **Phase Sync:** Ensure the **Druskel Carrier REF** is calibrated within 300ms of the loop initialization, or the interlaced data will decouple, causing a permanent loss of the variable state.
