## What it is
**PZL Bielsko SZD-30 *Pirat*** is a **Polish two‑seat training glider** (sailplane) designed by the **SZD (Szybowcowy Zakład Doświadczalny – Gliding Experimental Works)** design group at **Bielsko‑Biała** and **series‑built by PZL‑Bielsko**. It was intended primarily for **club training** (including progression beyond the very first dual instruction) and general utility flying.

You’ll see it referenced under a few closely related labels:
- **SZD-30 Pirat** (design/type designation is SZD-30; name is Pirat)
- **PZL-Bielsko Pirat** (manufacturer attribution in service/exports)

## Role and place in Polish gliding
Poland produced a long line of successful club and training gliders (e.g., Bocian, Puchacz, etc.). The **Pirat** sits in that tradition as a **dual-control trainer** used for:
- ab‑initio-to-intermediate instruction (depending on local syllabus)
- circuit practice and soaring introduction
- club “workhorse” flying (aerotow/winch launches, general handling)

Over time, more modern fiberglass trainers (notably later SZD designs) tended to replace wooden trainers like Pirat, but it remains a recognizable part of Polish—and exported—club fleets.

## General design features (typical of the type)
While individual aircraft can differ by production batch, repairs, and local modifications, the SZD-30 is generally characterized by:

### Seating and cockpit
- **Two seats in tandem** (student typically in front, instructor behind)
- **Dual controls**
- A **long, multi-panel canopy** typical of the era, giving good training visibility compared with older open-cockpit types

### Airframe construction
- Commonly described as **predominantly wooden construction** (plywood and wood structure), consistent with many Eastern European trainers of its generation.
- Wings typically use a **torsion-resistant leading edge (“D-box”)** with fabric/ply covering elsewhere (construction details can vary by source and by rebuild).

### Wing and control surfaces
- A **moderate-aspect-ratio wing** optimized for training/handling rather than maximum glide performance.
- **Spoilers/airbrakes** fitted for approach control (the exact style/arrangement is often described similarly to other European club gliders of the period).

### Landing gear
- A **fixed main wheel** arrangement with a skid/tail support is typical for club trainers of that era (exact fit can vary with refurbishment).

## Operational use
In service the Pirat is generally regarded as a solid **club trainer**: stable enough for instruction, with forgiving handling, and equipped for normal training launch methods:
- **Aerotow**
- **Winch launch** (where approved and equipped)

As with any older wooden sailplane, continued airworthiness tends to depend heavily on:
- quality of storage (humidity control matters)
- inspection regime (bond lines, spars, fittings)
- repair documentation and compliance with national continuing-airworthiness rules

## Production and distribution (high-level)
- Designed at **SZD in Bielsko‑Biała**
- Built by **PZL‑Bielsko**
- Used in **Poland** and also **exported** to a number of countries through the typical Eastern Bloc and broader club-market channels of the time (exact operator lists vary by registry and surviving airframes)

## Variants and designation notes
Public references most commonly center on **SZD‑30 “Pirat”** as the principal production identity. Some sources mention sub-variants (lettered suffixes) tied to incremental production changes or equipment fits; however, the naming is not always consistently presented across registries and historical summaries.

## What I can do next (if you want it)
If you want “everything” down to hard numbers and documents, tell me what level you need and I’ll tailor it. For example:
1) **Exact specifications** (span, area, aspect ratio, empty/max mass, best L/D, Vne, stall, etc.)  
2) **Production counts and years**, prototype vs series details  
3) **Flight manual/POH-level operating limitations** (aerobatics approvals if any, placards, CG range)  
4) **Airworthiness/maintenance** notes specific to wooden SZD trainers  

Also, if you share a link or an image of the data plate / registration entry, I can help identify the exact variant and likely configuration.
