## PZL Bielsko / SZD-30 **Pirat**

The **PZL Bielsko SZD-30 Pirat** is a Polish single-seat club sailplane/glider, best known as a rugged, forgiving, all-round soaring aircraft used for training, early cross-country flying, and club operations. “Pirat” means **“Pirate”** in Polish.

It was designed by the **SZD — Szybowcowy Zakład Doświadczalny** glider design bureau at **Bielsko-Biała**, Poland. Later, the Bielsko works became associated with the **PZL-Bielsko** name, so the aircraft is often referred to as the **PZL Bielsko SZD-30 Pirat**.

---

# Overview

| Item | Details |
|---|---|
| Type | Single-seat sailplane / club glider |
| Country | Poland |
| Manufacturer | SZD / PZL-Bielsko, Bielsko-Biała |
| Name | **Pirat** — “Pirate” |
| First flight | Mid-1960s, commonly cited as **1966** |
| Production | Late 1960s–1970s |
| Number built | Usually quoted at around **770–780 aircraft** |
| Role | Training, club soaring, early cross-country, general-purpose gliding |
| Construction | Mainly wood/fabric, with some composite/glass-fibre elements depending on version |
| Wingspan | 15 m class |
| Best glide | About **31:1** |

---

# Historical background

The SZD-30 was developed during a period when Polish glider design was highly respected internationally. SZD produced many important sailplanes, including the **Bocian**, **Mucha**, **Foka**, **Cobra**, and later the **Jantar** series.

The Pirat was intended as a **universal club glider**: more capable than basic trainers, but simpler, cheaper, and more robust than high-performance competition sailplanes. It came at a time when gliding clubs needed single-seat aircraft suitable for pilots progressing beyond two-seat training.

Although it had a 15 m wingspan and could be considered a Standard Class-type sailplane in layout, the Pirat was not a cutting-edge competition machine by the time glass-fibre sailplanes such as the Standard Cirrus, Libelle, and ASW 15 began to dominate. Instead, its real success came as a **reliable club aircraft**.

---

# Design and construction

The SZD-30 Pirat is a **single-seat, high-wing/shoulder-wing cantilever monoplane** with a conventional glider layout.

## Structure

The Pirat is primarily of **wooden construction**, typical of many 1950s and 1960s European gliders. The wing uses a wooden structure with plywood-covered leading sections and fabric covering over parts of the structure. The fuselage is also largely wooden, though some examples and production details include glass-fibre or composite components, especially around fairings or nose/cockpit areas depending on version and refurbishment.

## Wing

The wing is a 15 m, unflapped sailplane wing. It has:

- No flaps  
- Airbrakes/spoilers for glide-path control  
- Moderate aspect ratio  
- Low-to-moderate wing loading  
- Forgiving handling suitable for club pilots  

Its glide performance is good for a wooden club glider, but below that of later all-fibreglass Standard Class machines.

## Tail

The Pirat is usually described as having a **T-tail** or high-mounted horizontal stabilizer arrangement, a feature common on many later gliders.

## Landing gear

The aircraft has a simple glider undercarriage, typically:

- Fixed main wheel or semi-recessed monowheel arrangement  
- Nose skid or skid-type protection, depending on aircraft/configuration  
- Tail skid or tail bumper  

The gear is simple and robust, suited to grass airfield club operations.

## Controls

The aircraft has conventional glider controls:

- Ailerons  
- Elevator  
- Rudder  
- Airbrakes/spoilers  
- Tow release for winch and/or aerotow, depending on installation  

It is generally considered pleasant and predictable to fly.

---

# Performance

Published figures vary slightly by source and variant, but typical SZD-30 Pirat figures are approximately:

| Specification | Approximate value |
|---|---:|
| Crew | 1 |
| Wingspan | **15.0 m** |
| Length | About **6.8–6.9 m** |
| Wing area | About **13.8 m²** |
| Aspect ratio | About **16.3** |
| Empty weight | Around **255–265 kg** |
| Maximum takeoff weight | Around **370–390 kg** |
| Best glide ratio | About **31:1** |
| Minimum sink | Around **0.65–0.7 m/s** |
| Best glide speed | Roughly **80–85 km/h** |
| Stall speed | Roughly **55–60 km/h**, depending on weight |
| Never-exceed speed, VNE | Commonly around **250 km/h** |
| Typical winch launch speed limit | Lower than aerotow/VNE; depends on manual |
| Water ballast | No |

Because individual aircraft may have different national approvals, placards, and flight manuals, exact speeds and limits should always be checked against the aircraft’s own documentation.

---

# Flying qualities

The Pirat is generally regarded as:

- Stable  
- Forgiving  
- Honest in the stall  
- Suitable for low-hour solo pilots moving into single-seat soaring  
- Capable of modest cross-country flights  
- Strong enough for normal club use  
- Not especially fast by modern standards  

It is a good “step-up” aircraft from two-seat trainers or very basic single-seaters. It offers better performance than many primary training sailplanes but is simpler and less demanding than more advanced racing gliders.

Its glide ratio of around 31:1 makes it a respectable wooden club sailplane, comparable in broad role to aircraft such as the Schleicher Ka 6, though exact handling and performance differ.

---

# Operational use

The SZD-30 was widely used by gliding clubs in Poland and exported to many other countries. It became common in Central and Eastern Europe and also appeared in Western Europe and elsewhere.

Typical uses included:

- Post-solo single-seat training  
- Bronze/Silver badge flying  
- Thermalling practice  
- Local soaring  
- Early cross-country flights  
- Club competitions  
- Occasional basic aerobatic or advanced handling training, where permitted by the aircraft’s approval and flight manual  

Many examples are still airworthy, though they require careful maintenance due to age and wooden construction.

---

# Vari
