The **SZD-30 Pirat** (Pirate) is one of the most famous and successful Polish gliders, designed for club training and performance aerobatics. It was developed by the *Szybowcowy Zakład Doświadczalny* (Glider Experimental Works) in Bielsko-Biała.

Here is a comprehensive overview of the aircraft:

### 1. Development History
The SZD-30 was designed in the mid-1960s by **Jerzy Śmielkiewicz**. The goal was to create a "standard class" solo glider that was rugged enough for club use but capable enough for Silver and Gold badge cross-country flights. 

*   **First Flight:** May 19, 1966.
*   **Production:** Between 1967 and around 1980, approximately **813 units** were produced.
*   **Export:** It was a massive commercial success for Poland, exported to over 20 countries, including the UK, USA, Canada, and Australia.

### 2. Design and Construction
The Pirat is a high-wing, single-seat glider made primarily of **wood**.

*   **Structure:** It features a wooden semi-monocoque fuselage and a plywood-covered wing with a single spar.
*   **The Wing:** It has a distinctive "shoulder-wing" configuration. The inner wing is rectangular, while the outer panels are tapered. This design was intended to provide docile stall characteristics.
*   **Tail:** It uses a "T-tail" configuration (the horizontal stabilizer is mounted on top of the vertical fin), which protects the elevator from damage when landing in tall grass or crops.
*   **Cockpit:** Known for being relatively spacious and comfortable for its era, featuring a canopy that opens sideways.

### 3. Variants
There are two primary versions of the Pirat:
*   **SZD-30:** The original production version.
*   **SZD-30C:** An updated version introduced in the late 1970s. Key changes included a fiberglass-reinforced fuselage, a different canopy shape, smaller wheels, and improved control surfaces (specifically the ailerons).

### 4. Flight Characteristics and Performance
The Pirat is legendary for its **air brakes**. It uses multi-segment DFS-type brakes on both the upper and lower surfaces of the wings. They are incredibly effective, allowing for very steep landing approaches—a vital feature for "out-landings" in small farmers' fields.

**Technical Specifications:**
*   **Wingspan:** 15.0 meters (Standard Class)
*   **Length:** 6.86 meters
*   **Glide Ratio (L/D):** 33:1 at 83 km/h (52 mph)
*   **Minimum Sink Rate:** 0.7 m/s (138 ft/min)
*   **VNE (Never Exceed Speed):** 250 km/h (155 mph / 135 knots)
*   **Empty Weight:** approx. 260 kg

### 5. Training and Aerobatics
The SZD-30 is often the first single-seater a student pilot flies after "going solo" in a two-seater like the SZD-9 Bocian or the SZD-50 Puchacz. 
*   It is cleared for **basic aerobatics** (loops, stalls, spins, turns).
*   Its handling is described as "harmonized" but firm; it requires proper rudder input, making it an excellent teaching tool for developing "stick and rudder" skills.

### 6. Common Issues / Airworthiness
While beloved, the Pirat has faced some structural challenges in its old age:
*   **Gluing Issues:** Like many wooden gliders from that era, the type of glue used (synthetic resin) can degrade over decades.
*   **Airworthiness Directives (ADs):** There have been specific inspections mandated for the wing spar attachments and the tailplane mounting to ensure structural integrity. 
*   **Life Extension:** In some regions, the service life of the airframe is capped at a certain number of hours (usually 3,000 to 6,000) unless rigorous structural inspections are performed.

### 7. Legacy
The SZD-30 Pirat remains a common sight at gliding clubs throughout Europe. While modern fiberglass gliders (like the ASW-19 or LS4) have far higher performance, the Pirat is favored for its ruggedness, its ability to land in tight spaces, and its status as a "classic" of the wooden glider era. 

If you visit a Polish airfield today, you are almost guaranteed to see a Pirat—usually painted in a classic white scheme with red or blue accents—waiting on the flight line.
