# PZL Bielsko SZD-30 Pirat

The SZD-30 Pirat ("Pirate") is a Polish single-seat glider designed for training and club use. It became one of the most successful and widely-produced Polish gliders, serving as a standard intermediate trainer in flying clubs across the Eastern Bloc and beyond.

## Design and Development

The Pirat was designed by Jerzy Śmielkiewicz at the Szybowcowy Zakład Doświadczalny (SZD - Glider Experimental Works) in Bielsko-Biała, Poland. The prototype first flew on **May 19, 1966**, and series production began in 1967.

It was conceived as a successor to the SZD-22 Mucha Standard, intended to fill the gap between basic trainers and high-performance sailplanes. The design emphasized ease of construction, simple handling, low cost, and durability — making it ideal for ab-initio post-solo training.

## Construction

- **Material:** All-wooden construction (pine and plywood) with fabric covering on control surfaces
- **Fuselage:** Semi-monocoque plywood structure
- **Wing:** Cantilever shoulder-mounted wing with a single main spar, featuring NACA 43012A and NACA 43010A airfoils
- **Tail:** Conventional tailplane with elevator and rudder
- **Landing gear:** Fixed monowheel with rubber shock absorption, plus nose skid and tail skid (some versions had a retractable wheel)
- **Airbrakes:** Schempp-Hirth type on upper and lower wing surfaces

## Specifications

- **Wingspan:** 15.0 m (49 ft 2 in)
- **Length:** 6.83 m (22 ft 5 in)
- **Wing area:** 13.8 m²
- **Aspect ratio:** 16.3
- **Empty weight:** ~245 kg
- **Max takeoff weight:** ~370 kg
- **Maximum L/D (glide ratio):** ~30:1 at ~85 km/h
- **Minimum sink:** ~0.75 m/s
- **Stall speed:** ~60 km/h
- **VNE (never exceed):** 200 km/h

## Variants

- **SZD-30 Pirat** – Original production version
- **SZD-30A** – Modified version with various improvements
- **SZD-30B** – Further refinements (some sources list this designation)

## Production and Service

Approximately **750 units** were built between 1967 and 1978, making it one of the most-produced Polish glider designs. It was exported widely to countries including the USSR, East Germany, Czechoslovakia, Hungary, Bulgaria, Yugoslavia, Finland, the United Kingdom, and various others.

The Pirat was used for:
- Cross-country training
- Cloud flying training (some equipped with appropriate instruments)
- Aerobatics (limited)
- Club racing

## Achievements and Legacy

The Pirat became the workhorse of Eastern European gliding clubs through the 1970s and 1980s. It was praised for its honest handling characteristics, forgiving stall behavior, and respectable performance for its category. Many examples remained airworthy into the 21st century, particularly with vintage glider enthusiasts.

The design philosophy — a robust, affordable, all-wood Standard Class glider — was eventually superseded by fiberglass designs like the SZD-41 Jantar Standard and SZD-48 Jantar Standard 2, but the Pirat remains a beloved classic in the gliding community.
