The **PZL Bielsko SZD-30 Pirat** was a **single-seat Polish Standard Class sailplane** developed in the 1960s. Here’s a compact but broad overview.

## Identity
- **Full designation:** **SZD-30 Pirat**
- **Manufacturer:** **SZD (Szybowcowy Zakład Doświadczalny)**, later associated with **PZL Bielsko**
- **Country:** Poland
- **Type:** Standard Class glider / sailplane
- **Era:** Designed and built in the 1960s

## Role and concept
The Pirat was intended as a **modern club and competition sailplane** for the FAI Standard Class, which generally meant:
- no flaps
- fixed landing gear arrangements within class rules
- emphasis on efficient soaring performance with manageable handling

It served as a step up from earlier wood-and-fabric gliders and reflected the shift toward **fiberglass composite** structures.

## Design features
General characteristics commonly associated with the SZD-30:
- **Single-seat**
- **High-wing sailplane layout**
- **T-tail**
- **Standard Class proportions**
- **Retractable or semi-recessed main wheel arrangement** depending on subvariant/details cited by source
- **Airbrakes / spoilers** for glidepath control
- **Composite construction**, especially fiberglass, though exact material breakdown can vary by production batch and documentation source

The aircraft had a relatively clean, modern appearance for its time and was considered one of Poland’s significant early fiberglass sailplanes.

## Development background
The Pirat emerged during a period when glider manufacturers across Europe were moving from traditional materials to composites. Poland’s SZD design bureau was very active in this transition and produced many influential sailplanes.

The SZD-30 was part of a family line of Polish sailplane designs that aimed to remain internationally competitive. It was followed and overshadowed by later, better-known Polish high-performance designs, but the Pirat remained important as a practical and widely used machine.

## Performance and reputation
The Pirat was generally regarded as:
- **pleasant to fly**
- **competent in club and regional competition use**
- **not among the absolute top performers** once newer generations of Standard Class ships appeared

In short, it was a respectable and useful glider rather than a dominant world-beater.

## Production and export
- Built in **significant numbers** for a Polish sailplane
- **Exported** to a number of countries
- Used in **gliding clubs**, training progression, badge flying, and competition

Polish gliders from SZD often had strong export success thanks to reasonable cost and solid handling, and the Pirat fit that pattern.

## Variants
The **SZD-30** had subvariants, and references may mention different suffixes. Documentation varies somewhat, but commonly encountered designations include:
- **SZD-30**
- **SZD-30C Pirat**
There were development and certification changes across the line.

## Approximate specifications
Figures can vary by source and variant, but typical numbers for the Pirat are roughly:

- **Wingspan:** about **15 m**
- **Length:** about **6.7–7.0 m**
- **Empty weight:** roughly **230–260 kg**
- **Maximum takeoff weight:** roughly **350–380 kg**
- **Best glide ratio:** around **34:1 to 36:1**
- **Minimum sink:** around **0.75–0.85 m/s**
- **Max speed:** often cited in the **around 190–200 km/h class**, depending on operating limitations

These numbers place it in the expected range for a 1960s Standard Class fiberglass glider.

## Operational use
Typical use included:
- thermal soaring
- cross-country flights
- club competition
- pilot progression into higher-performance sailplanes

It was not primarily a basic trainer, but clubs could use it for experienced solo pilots transitioning into modern single-seaters.

## Historical significance
The Pirat matters because it represents:
1. **Poland’s early composite sailplane development**
2. **the maturation of SZD as an internationally recognized glider design house**
3. **the evolution of Standard Class sailplanes in the 1960s**

Even if later designs surpassed it, it remains part of the important bridge between earlier wooden gliders and later high-performance composite sailplanes.

## Naming
“**Pirat**” means **“Pirate”** in Polish.

## Things that are often confused
A few caveats:
- Sources sometimes mix **SZD bureau design numbers**, **PZL Bielsko manufacturing references**, and **variant suffixes**
- Performance figures can differ depending on:
  - variant
  - wing modifications
  - source language
  - whether data are measured or promotional
- Some online summaries overgeneralize the exact construction or landing gear arrangement

## Bottom line
The **PZL Bielsko SZD-30 Pirat** was a **Polish 15-meter Standard Class single-seat sailplane**, introduced in the **1960s**, notable as an **early fiberglass/composite SZD design**. It was **widely used, exported, and well regarded**, though eventually outclassed by newer sailplanes.

If you want, I can also give you:
1. a **detailed technical spec sheet**,
2. a **variant-by-variant breakdown**, or
3. a **history of the Pirat’s design and operational use**.
